{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":125,"n_cols":8,"rows_kept":125,"cut":false,"hidden":false,"merged":[]}
["序号","数据库字段","中文名","索引","所有“率”保留4位小数"]
[0,"rpt_time",null,1,"sdate"]
[1,"user_label","对象名称",3]
[2,"nci","对象编号",2,"enbid*4096+cell_id"]
[3,"enbid",null,null,"为空过滤，对象编号中间部分"]
[4,"cell_id",null,null,"为空过滤，对象编号末尾"]
[5,"enb_cell",null,null,"3_4"]
[6,"vendor","厂商名称",6]
[7,"gnb_rrc_conn_ratio","RRC建立成功率(%)",10]
[8,"gnb_flow_conn_ratio","QoSFlow建立成功率",18]
[9,"gnb_wireless_conn_ratio","无线接入成功率",14]
[10,"gnb_wireless_drop_ratio","UE上下文掉线率",23]
[11,"gnb_sw_succ_ratio","5G切换成功率(%)",79]
[12,"kpi_rlcupoctul","上行RLC层用户面流量",59]
[13,"kpi_rlcupoctdl","下行RLC层用户面流量",60]
[14,"gnb_ul_prb_use_ratio","小区上行PRB平均占用率",53]
[15,"gnb_dl_prb_use_ratio","小区下行PRB平均占用率",56]
[16,"kpi_pdcchcceoccupancyrate","PDCCH信道CCE占用率",80]
[17,"kpi_ngsig_succconnrate","NG接口信令连接建立成功率",11]
[18,"kpi_flowdroprate_celllevel","Flow掉线率（小区级）",81]
[19,"kpi_rrcconnreestabrate","RRC连接重建比率",82]
[20,"kpi_hosuccoutintergnbrate_ng","gNB间NG切换成功率",83]
[21,"kpi_hosuccoutintergnbrate_xn","gNB间Xn切换成功率",84]
[22,"kpi_hosuccoutintergnbrate","gNB间切换成功率",85]
[23,"kpi_hosuccoutintragnbrate","gNB内切换成功率",86]
[24,"kpi_hosuccoutrate_intrafreq","同频切换执行成功率",87]
[25,"kpi_hosuccoutrate_interfreq","异频切换执行成功率",88]
[26,"kpi_rlcnbrpktlossratedl","小区RLC层下行丢包率",89]
[27,"kpi_macblerul","MAC层上行误块率",90]
[28,"kpi_macblerdl","MAC层下行误块率",91]
[29,"kpi_harqretransrateul","上行HARQ重传比率",92]
[30,"kpi_harqretransratedl","下行HARQ重传比率",93]
[31,"kpi_rank2percentdl","下行双流占比",94]
[32,"kpi_rank3percentdl","下行3流占比",95]
[33,"kpi_rank4percentdl","下行4流占比",96]
[34,"kpi_qpskpercentul","上行QPSK编码比例",97]
[35,"kpi_16qampercentul","上行16QAM编码比例",98]
[36,"kpi_64qampercentul","上行64QAM编码比例",99]
[37,"kpi_256qampercentul","上行256QAM编码比例",100]
[38,"kpi_qpskpercentdl","下行QPSK编码比例",101]
[39,"kpi_16qampercentdl","下行16QAM编码比例",102]
[40,"kpi_64qampercentdl","下行64QAM编码比例",103]
[41,"kpi_256qampercentdl","下行256QAM编码比例",104]
[42,"kpi_dtchprbassnrateul","上行PUSCH信道PRB平均利用率",62]
[43,"kpi_dtchprbassnratedl","下行PDSCH信道PRB平均利用率",63]
[44,"kpi_avgthrouperprbul","上行每PRB平均吞吐量",105]
[45,"kpi_avgthrouperprbdl","下行每PRB平均吞吐量",106]
[46,"kpi_pdcpupoctul","上行PDCP层用户面流量",57]
[47,"kpi_pdcpupoctdl","下行PDCP层用户面流量",58]
[48,"averagelayersul","上行MIMO平均配对层数",107]
[49,"averagelayersdl","下行MIMO平均配对层数",108]
[50,"mupairprbrateul","上行MIMO配对PRB占比",109]
[51,"mupairprbratedl","下行MIMO配对PRB占比",110]
[52,"context_attinitalsetup","初始上下文建立请求次数",111]
[53,"context_succinitalsetup","初始上下文建立成功次数",112]
[54,"context_failinitalsetup","初始上下文建立失败次数",113]
[55,"rrc_succconnestab","RRC建立成功次数(次)",8]
[56,"rrc_attconnestab","RRC建立请求次数(次)",7]
[57,"flow_nbrsuccestab","QoSFlow建立成功数",20]
[58,"flow_nbrattestab","QoSFlow建立请求数",19]
[59,"ngsig_connestabsucc","NG接口信令连接建立成功次数",12]
[60,"ngsig_connestabatt","NG接口信令连接建立请求次数",13]
[61,"context_attrelgnb","gNB请求释放上下文数",114]
[62,"context_attrelgnb_normal","正常的gNB请求释放上下文数",115]
[63,"context_nbrleft","遗留上下文个数",116]
[64,"ho_succexecinc","切换入成功次数",117]
[65,"rrc_succconnreestab_nonsrccell","RRC连接重建成功次数(非源侧小区)",118]
[66,"ho_succoutintercung","gNB间NG切换出成功次数",119]
[67,"ho_succoutintercuxn","gNB间Xn切换出成功次数",120]
[68,"ho_succoutintracuinterdu","CU内DU间切换出执行成功次数",121]
[69,"ho_succoutintradu","CU内DU内切换出成功次数",122]
[70,"ho_attoutintercung","gNB间NG切换出准备请求次数",123]
[71,"ho_attoutintercuxn","gNB间Xn切换出准备请求次数",124]
[72,"ho_attoutintracuinterdu","CU内DU间切换出执行请求次数",125]
[73,"ho_attoutcuintradu","CU内DU内切换出执行请求次数",126]
[74,"rlc_upoctul","上行RLC层用户面流量",59]
[75,"rlc_upoctdl","下行RLC层用户面流量",60]
[76,"rru_puschprbassn","上行PUSCH PRB占用数",127]
[77,"rru_puschprbtot","上行PUSCH PRB可用数",128]
[78,"rru_pdschprbassn","下行PDSCH PRB占用数",129]
[79,"rru_pdcchcceutil","PDCCH信道CCE占用个数",130]
[80,"rru_pdcchcceavail","PDCCH信道CCE可用个数",131]
[81,"flow_nbrreqrelgnb","gNB请求释放的Flow数",132]
[82,"flow_nbrreqrelgnb_normal","正常的gNB请求释放的Flow数",133]
[83,"flow_hoadmitfail","切出接纳失败的Flow数",134]
[84,"flow_nbrleft","遗留Flow个数",135]
[85,"flow_nbrhoinc","切换入Flow数",136]
[86,"rrc_attconnreestab","RRC连接重建请求次数",137]
[87,"ho_succoutintrafreq","同频切换出成功次数",138]
[88,"ho_attoutexecintrafreq","同频切换出执行请求次数",139]
[89,"ho_succoutinterfreq","异频切换出成功次数",140]
[90,"ho_attoutexecinterfreq","异频切换出执行请求次数",141]
[91,"rlc_nbrpktlossdl","小区下行RLC SDU丢包数",142]
[92,"rlc_nbrpktdl","小区下行RLC SDU发送包数",143]
[93,"mac_nbrreserrtbul","上行残留错误TB数",144]
[94,"mac_nbrinittbul","上行传输初始TB数",145]
[95,"mac_nbrreserrtbdl","下行残留错误TB数",147]
[96,"mac_nbrtbdl","下行传输TB数",148]
[97,"mac_nbrinittbdl","下行传输初始TB数",149]
[98,"mac_nbrtbdl_rank2","双流下行传输TB数",150]
[99,"mac_nbrtbdl_rank3","3流下行传输TB数",151]
[100,"mac_nbrtbdl_rank4","4流下行传输TB数",152]
[101,"mac_nbrinittbul_qpsk","QPSK模式上行传输初始TB数",153]
[102,"mac_nbrinittbul_16qam","16QAM模式上行传输初始TB数",154]
[103,"mac_nbrinittbul_64qam","64QAM模式上行传输初始TB数",155]
[104,"mac_nbrinittbul_256qam","256QAM模式下行传输初始TB数",156]
[105,"mac_nbrinittbdl_qpsk","QPSK模式下行传输初始TB数",157]
[106,"mac_nbrinittbdl_16qam","16QAM模式下行传输初始TB数",158]
[107,"mac_nbrinittbdl_64qam","64QAM模式下行传输初始TB数",159]
[108,"mac_nbrinittbdl_256qam","256QAM模式下行传输初始TB数",160]
[109,"rru_dtchprbassnul","上行业务信道占用PRB数",161]
[110,"rru_dtchprbassndl","下行业务信道占用PRB数",162]
[111,"rru_pdschprbtot","下行PDSCH PRB可用数",163]
[112,"mac_cpoctul","小区MAC层传输成功的上行流量",164]
[113,"mac_cpoctdl","小区MAC层传输成功的下行流量",165]
[114,"pdcp_upoctul","上行PDCP层用户面流量",57,null,"kpi_pdcpupoctul","上行PDCP层用户面流量",57]
[115,"pdcp_upoctdl","下行PDCP层用户面流量",58,null,"kpi_pdcpupoctdl","下行PDCP层用户面流量",58]
[116,"phy_ulmeannl_prb","小区上行每PRB平均干扰电平",41]
[117,"phy_ulmaxnl_prb","小区RB上行最大干扰电平",166]
[118,"rrc_redirecttolte","RRC 重定向到LTE次数",167]
[119,"rrc_redirecttolte_epsfb","EPS fallback RRC 重定向到LTE次数",168]
[120,"rrc_sannsaconnusermean","小区平均用户数",169]
[121,"rrc_sannsaconnusermax","最大用户数",65]
[122,"rrc_connmean","用户数均值",64]
[123,"rrc_connmax","RRC连接最大用户数",61]