{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":129,"n_cols":7,"rows_kept":129,"cut":false,"hidden":false,"merged":[]}
["中文表名",null,null,"英文表名","备注信息"]
["资源域_性能_5G无线指标_共享1_小时",null,null,"DW_FT_RE_ST_NRCELL_SHR1_H","资源域_性能_5G无线指标_共享1_小时"]
["中文字段名","PM解析数据库现有字段","沃网络现有字段","英文字段名","字段类型","字段描述","算法描述"]
["时间","分析时间","分析时间","STAT_TIME","DATE","时间"]
["网元名称","对象名称","对象名称","USER_LABEL","VARCHAR2(128)","网元名称","USER_LABEL"]
["小区唯一标识","对象编号","对象编号","NCI","NUMBER","小区唯一标识"]
["基站ID",null,null,"GENBID","NUMBER","基站ID"]
["5G-RRC连接建立成功率","RRC建立成功率(%)","rrc连接建立成功率","GNB_RRC_CONN_RATIO","NUMBER","5G-RRC连接建立成功率","RRC_SuccConnEstab/RRC_AttConnEstab*100%"]
["5G-QoS Flow建立成功率","QoSFlow建立成功率","qosflow建立成功率","GNB_FLOW_CONN_RATIO","NUMBER","5G-QoS Flow建立成功率","Flow_NbrSuccEstab/Flow_NbrAttEstab"]
["5G无线接通率(%)","无线接入成功率","无线接入成功率","GNB_WIRELESS_CONN_RATIO","NUMBER","5G无线接通率(%)","(RRC_SuccConnEstab/RRC_AttConnEstab)*(Flow_NbrSuccEstab/Flow_NbrAttEstab)*(NGSIG_ConnEstabSucc/NGSIG_ConnEstabAtt)"]
["5G无线掉线率(%)",null,"ue上下文掉线率","GNB_WIRELESS_DROP_RATIO","NUMBER","5G无线掉线率(%)","(CONTEXT_AttRelgNB-CONTEXT_AttRelgNB_Normal)/(CONTEXT_SuccInitalSetup+CONTEXT_NbrLeft+HO_SuccExecInc+RRC_SuccConnReestab_NonSrccell)"]
["5G切换成功率(%)",null,"系统内切换成功率","GNB_SW_SUCC_RATIO","NUMBER","5G切换成功率(%)","(HO_SuccOutInterCuNG+HO_SuccOutInterCuXn+HO_SuccOutIntraCUInterDU+HO_SuccOutIntraDU)/(HO_AttOutInterCuNG+HO_AttOutInterCuXn+HO_AttOutIntraCUInterDU+HO_AttOutCUIntraDU)"]
["RLC层上行业务字节数(MB)","上行RLC层用户面流量","上行rlc层用户面流量","KPI_RLCUPOCTUL","NUMBER","RLC层上行业务字节数(MB)","RLC_UpOctUl/1000"]
["RLC层下行业务字节数(MB)","下行RLC层用户面流量","下行rlc层用户面流量","KPI_RLCUPOCTDL","NUMBER","RLC层下行业务字节数(MB)","RLC_UpOctDl/1000"]
["5G上行PRB平均利用率(%)","小区上行PRB平均占用率","小区上行prb平均占用率","GNB_UL_PRB_USE_RATIO","NUMBER","5G上行PRB平均利用率(%)","RRU_PuschPrbAssn/RRU_PuschPrbTot"]
["5G下行PRB平均利用率(%)","小区下行PRB平均占用率","小区下行prb平均占用率","GNB_DL_PRB_USE_RATIO","NUMBER","5G下行PRB平均利用率(%)","RRU_PdschPrbAssn/RRU_PdschPrbTot"]
["PDCCH信道CCE占用率",null,"pdcch信道cce占用个数/pdcch信道cce可用个数","KPI_PDCCHCCEOCCUPANCYRATE","NUMBER","PDCCH信道CCE占用率","RRU_PdcchCceUtil/RRU_PdcchCceAvail*100"]
["NG接口UE相关逻辑信令连接建立成功率","NG接口信令连接建立成功率","ng接口信令连接建立成功率","KPI_NGSIG_SUCCCONNRATE","NUMBER","NG接口UE相关逻辑信令连接建立成功率","NGSIG_ConnEstabSucc/NGSIG_ConnEstabAtt*100%"]
["Flow掉线率（小区级）",null,"qosflow掉线率","KPI_FLOWDROPRATE_CELLLEVEL","NUMBER","Flow掉线率（小区级）","(Flow_NbrReqRelGnb -Flow_NbrReqRelGnb_Normal +Flow_HoAdmitFail) / ( Flow_NbrLeft +Flow_NbrSuccEstab +Flow_NbrHoInc ) *100%"]
["RRC连接重建比率\r",null,"rrc重建比例","KPI_RRCCONNREESTABRATE","NUMBER","RRC连接重建比率","RRC_AttConnReestab/（RRC_AttConnReestab+RRC_AttConnEstab）*100%"]
["gNB间NG切换成功率\r",null,"ng接口站间切换成功率","KPI_HOSUCCOUTINTERGNBRATE_NG","NUMBER","gNB间NG切换成功率\r","HO_SuccOutInterCuNG\r/HO_AttOutInterCuNG*100%"]
["gNB间Xn切换成功率\r",null,"xn接口站间切换成功率","KPI_HOSUCCOUTINTERGNBRATE_XN","NUMBER","gNB间Xn切换成功率\r","HO_SuccOutInterCuXn/\rHO_AttOutInterCuXn*100%"]
["gNB间切换成功率",null,"站间切换成功率","KPI_HOSUCCOUTINTERGNBRATE","NUMBER","gNB间切换成功率","( (HO_SuccOutInterCuNG+HO_SuccOutInterCuXn\n)/(HO_AttOutInterCuNG+HO_AttOutInterCuXn ) *100%"]
["gNB内切换成功率",null,"gnb站内切换成功率","KPI_HOSUCCOUTINTRAGNBRATE","NUMBER","gNB内切换成功率","（HO_SuccOutIntraCUInterDU+HO_SuccOutIntraDU）/（HO_AttOutIntraCUInterDU+HO_AttOutCUIntraDU）\r*100%"]
["同频切换执行成功率\r",null,"同频切换成功率","KPI_HOSUCCOUTRATE_INTRAFREQ","NUMBER","同频切换执行成功率\r","HO_SuccOutIntraFreq\n/HO_AttOutExecIntraFreq*100%"]
["异频切换执行成功率\r",null,"异频切换成功率","KPI_HOSUCCOUTRATE_INTERFREQ","NUMBER","异频切换执行成功率\r","HO_SuccOutInterFreq\n\r/HO_AttOutExecInterFreq*100%"]
["小区RLC层下行丢包率",null,"下行rlc层用户面丢包率","KPI_RLCNBRPKTLOSSRATEDL","NUMBER","小区RLC层下行丢包率","RLC_NbrPktLossDl/RLC_NbrPktDl*100%"]
["MAC层上行误块率",null,"上行mac层传输误块率","KPI_MACBLERUL","NUMBER","MAC层上行误块率","MAC_NbrResErrTbUl/MAC_NbrInitTbUl*100%"]
["MAC层下行误块率",null,"下行mac层传输误块率","KPI_MACBLERDL","NUMBER","MAC层下行误块率","MAC_NbrResErrTbDl/MAC_NbrInitTbDl*100%"]
["上行HARQ重传比率",null,"上行harq重传比率","KPI_HARQRETRANSRATEUL","NUMBER","上行HARQ重传比率","（MAC_NbrTbUl-MAC_NbrInitTbUl）/MAC_NbrTbUl*100%"]
["下行HARQ重传比率",null,"下行harq重传比率","KPI_HARQRETRANSRATEDL","NUMBER","下行HARQ重传比率","（MAC_NbrTbDl-MAC_NbrInitTbDl）/MAC_NbrTbDl*100%"]
["下行双流占比",null,"下行双流占比","KPI_RANK2PERCENTDL","NUMBER","下行双流占比","（MAC_NbrTbDl_Rank2/MAC_NbrTbDl）*100%"]
["下行3流占比",null,"下行三流占比","KPI_RANK3PERCENTDL","NUMBER","下行3流占比","（MAC_NbrTbDl_Rank3/MAC_NbrTbDl）*100%"]
["下行4流占比",null,"下行四流占比","KPI_RANK4PERCENTDL","NUMBER","下行4流占比","（MAC_NbrTbDl_Rank4/MAC_NbrTbDl）*100%"]
["上行QPSK编码比例",null,null,"KPI_QPSKPERCENTUL","NUMBER","上行QPSK编码比例","MAC_NbrInitTbUl_Qpsk/MAC_NbrInitTbUl*100%"]
["上行16QAM编码比例",null,null,"KPI_16QAMPERCENTUL","NUMBER","上行16QAM编码比例","MAC_NbrInitTbUl_16Qam/MAC_NbrInitTbUl*100%"]
["上行64QAM编码比例",null,null,"KPI_64QAMPERCENTUL","NUMBER","上行64QAM编码比例","MAC_NbrInitTbUl_64Qam/MAC_NbrInitTbUl*100%"]
["上行256QAM编码比例",null,null,"KPI_256QAMPERCENTUL","NUMBER","上行256QAM编码比例","MAC_NbrInitTbUl_256Qam/MAC_NbrInitTbUl*100%"]
["下行QPSK编码比例",null,null,"KPI_QPSKPERCENTDL","NUMBER","下行QPSK编码比例","MAC_NbrInitTbDl_Qpsk/MAC_NbrInitTbDl*100%"]
["下行16QAM编码比例",null,null,"KPI_16QAMPERCENTDL","NUMBER","下行16QAM编码比例","MAC_NbrInitTbDl_16Qam/MAC_NbrInitTbDl*100%"]
["下行64QAM编码比例",null,null,"KPI_64QAMPERCENTDL","NUMBER","下行64QAM编码比例","MAC_NbrInitTbDl_64Qam/MAC_NbrInitTbDl*100%"]
["下行256QAM编码比例",null,null,"KPI_256QAMPERCENTDL","NUMBER","下行256QAM编码比例","MAC_NbrInitTbDl_256Qam/MAC_NbrInitTbDl*100%"]
["上行业务信息PRB占用率\r","上行PUSCH信道PRB平均利用率","上行pusch信道prb平均利用率","KPI_DTCHPRBASSNRATEUL","NUMBER","上行业务信息PRB占用率\r","RRU_DtchPrbAssnUl/RRU_PuschPrbTot*100%"]
["下行业务信息PRB占用率\r","下行PDSCH信道PRB平均利用率","下行pdsch信道prb平均利用率","KPI_DTCHPRBASSNRATEDL","NUMBER","下行业务信息PRB占用率\r","RRU_DtchPrbAssnDl/RRU_PdschPrbTot*100%"]
["上行每PRB平均吞吐量",null,null,"KPI_AVGTHROUPERPRBUL","NUMBER","上行每PRB平均吞吐量","MAC_CpOctUl*8/RRU_DtchPrbAssnUl"]
["下行每PRB平均吞吐量",null,null,"KPI_AVGTHROUPERPRBDL","NUMBER","下行每PRB平均吞吐量","MAC_CpOctDl*8/RRU_DtchPrbAssnDl"]
["PDCP上行业务字节数\r","上行PDCP层用户面流量","上行pdcp层用户面流量","KPI_PDCPUPOCTUL","NUMBER","PDCP上行业务字节数\r","PDCP_UpOctUl/1000"]
["PDCP下行业务字节数\r","下行PDCP层用户面流量","下行pdcp层用户面流量","KPI_PDCPUPOCTDL","NUMBER","PDCP下行业务字节数\r","PDCP_UpOctDl/1000"]
["上行MIMO平均配对层数",null,"上行mu-mimo平均配对层数","KPI.AverageLayersUl","NUMBER","上行MIMO平均配对层数","sum(MAC.NbrRbUlMassiveMimoSM.2*2 ...MAC.NbrRbUlMassiveMimoSM.n*n)/sum(MAC.NbrRbUlMassiveMimoSM.2...MAC.NbrRbUlMassiveMimoSM.n)"]
["下行MIMO平均配对层数",null,"下行mu-mimo平均配对层数","KPI.AverageLayersDl","NUMBER","下行MIMO平均配对层数","sum(MAC.NbrRbDlMassiveMimoSM.2*2 ...MAC.NbrRbDlMassiveMimoSM.n*n)/sum(MAC.NbrRbDlMassiveMimoSM.2 ...MAC.NbrRbDlMassiveMimoSM.n)"]
["上行MIMO配对PRB占比",null,"上行业务信道mimo配对prb占比","KPI.MUPairPrbRateUl","NUMBER","上行MIMO配对PRB占比","sum(MAC.NbrRbUlMassiveMimoSM.2+...+MAC.NbrRbUlMassiveMimoSM.n)/sum(MAC.NbrRbUlMassiveMimoSM.1...MAC.NbrRbUlMassiveMimoSM.n)*100%"]
["下行MIMO配对PRB占比",null,"下行业务信道mimo配对prb占比","KPI.MUPairPrbRateDl","NUMBER","下行MIMO配对PRB占比","sum(MAC.NbrRbDlMassiveMimoSM.2+...+MAC.NbrRbDlMassiveMimoSM.n)/sum(MAC.NbrRbDlMassiveMimoSM.1+...+MAC.NbrRbDlMassiveMimoSM.n)*100%"]
["初始上下文建立请求次数",null,"ue上下文建立请求次数","CONTEXT_AttInitalSetup","NUMBER","初始上下文建立请求次数","CONTEXT.AttInitalSetup"]
["初始上下文建立成功次数",null,"ue上下文建立成功次数","CONTEXT_SuccInitalSetup","NUMBER","初始上下文建立成功次数","CONTEXT.SuccInitalSetup"]
["初始上下文建立失败次数",null,"ue上下文建立成功率","CONTEXT_FailInitalSetup","NUMBER","初始上下文建立失败次数","CONTEXT.FailInitalSetup"]
["RRC连接建立成功次数","RRC建立成功次数(次)","rrc连接建立成功次数","RRC_SuccConnEstab","NUMBER","RRC连接建立成功次数","RRC.SuccConnEstab"]
["RRC连接建立请求次数","RRC建立请求次数(次)","rrc连接建立请求次数","RRC_AttConnEstab","NUMBER","RRC连接建立请求次数","RRC.AttConnEstab"]
["Flow建立成功数","QoSFlow建立成功数","qosflow建立成功数","Flow_NbrSuccEstab","NUMBER","Flow建立成功数","Flow.NbrSuccEstab"]
["Flow建立请求数","QoSFlow建立请求数","qosflow建立请求数","Flow_NbrAttEstab","NUMBER","Flow建立请求数","Flow.NbrAttEstab"]
["NG接口UE相关逻辑信令连接建立成功次数","NG接口信令连接建立成功次数","ng接口信令连接建立成功次数","NGSIG_ConnEstabSucc","NUMBER","NG接口UE相关逻辑信令连接建立成功次数","NGSIG.ConnEstabSucc"]
["NG接口UE相关逻辑信令连接建立请求次数","NG接口信令连接建立请求次数","ng接口信令连接建立请求次数","NGSIG_ConnEstabAtt","NUMBER","NG接口UE相关逻辑信令连接建立请求次数","NGSIG.ConnEstabAtt"]
["gNB请求释放上下文数",null,"gnb发起的ue上下文释放次数","CONTEXT_AttRelgNB","NUMBER","gNB请求释放上下文数","CONTEXT.AttRelgNB"]
["正常的gNB请求释放上下文数",null,"gnb发起的ue上下文正常释放次数","CONTEXT_AttRelgNB_Normal","NUMBER","正常的gNB请求释放上下文数","CONTEXT.AttRelgNB.Normal"]
["遗留上下文个数",null,null,"CONTEXT_NbrLeft","NUMBER","遗留上下文个数","CONTEXT.NbrLeft"]
["切换入成功次数",null,null,"HO_SuccExecInc","NUMBER","切换入成功次数","HO.SuccExecInc"]
["RRC连接重建成功次数(非源侧小区)",null,"rrc重建完成次数","RRC_SuccConnReestab_NonSrccell","NUMBER","RRC连接重建成功次数(非源侧小区)","RRC.SuccConnReestab.NonSrccell"]
["gNB间NG切换出成功次数",null,"ng接口站间切换成功次数","HO_SuccOutInterCuNG","NUMBER","gNB间NG切换出成功次数","HO.SuccOutInterCuNG"]
["gNB间Xn切换出成功次数",null,"xn接口站间切换成功次数","HO_SuccOutInterCuXn","NUMBER","gNB间Xn切换出成功次数","HO.SuccOutInterCuXn"]
["CU内DU间切换出执行成功次数",null,null,"HO_SuccOutIntraCUInterDU","NUMBER","CU内DU间切换出执行成功次数","HO.SuccOutIntraCUInterDU"]
["CU内DU内切换出成功次数",null,null,"HO_SuccOutIntraDU","NUMBER","CU内DU内切换出成功次数","HO.SuccOutIntraDU"]
["gNB间NG切换出准备请求次数",null,"ng接口站间切换请求次数","HO_AttOutInterCuNG","NUMBER","gNB间NG切换出准备请求次数","HO.AttOutInterCuNG"]
["gNB间Xn切换出准备请求次数",null,"xn接口站间切换请求次数","HO_AttOutInterCuXn","NUMBER","gNB间Xn切换出准备请求次数","HO.AttOutInterCuXn"]
["CU内DU间切换出执行请求次数",null,null,"HO_AttOutIntraCUInterDU","NUMBER","CU内DU间切换出执行请求次数","HO.AttOutIntraCUInterDU"]
["CU内DU内切换出执行请求次数",null,null,"HO_AttOutCUIntraDU","NUMBER","CU内DU内切换出执行请求次数","HO.AttOutCUIntraDU"]
["小区上行RLC SDU接收字节数","上行RLC层用户面流量","上行rlc层用户面流量","RLC_UpOctUl","NUMBER","小区上行RLC SDU接收字节数","RLC.UpOctUl"]
["小区下行RLC SDU发送字节数","下行RLC层用户面流量","下行rlc层用户面流量","RLC_UpOctDl","NUMBER","小区下行RLC SDU发送字节数","RLC.UpOctDl"]
["上行PUSCH PRB占用数",null,"上行pusch信道prb占用平均数","RRU_PuschPrbAssn","NUMBER","上行PUSCH PRB占用数","RRU.PuschPrbAssn"]
["上行PUSCH PRB可用数",null,"上行pusch信道prb可用数","RRU_PuschPrbTot","NUMBER","上行PUSCH PRB可用数","RRU.PuschPrbTot"]
["下行PDSCH PRB占用数",null,"下行pdsch信道prb占用平均数","RRU_PdschPrbAssn","NUMBER","下行PDSCH PRB占用数","RRU.PdschPrbAssn"]
["PDCCH信道CCE占用个数",null,"pdcch信道cce占用个数","RRU_PdcchCceUtil","NUMBER","PDCCH信道CCE占用个数","RRU.PdcchCceUtil"]
["PDCCH信道CCE可用个数",null,"pdcch信道cce可用个数","RRU_PdcchCceAvail","NUMBER","PDCCH信道CCE可用个数","RRU.PdcchCceAvail"]
["gNB请求释放的Flow数",null,"gnb发起的qosflow释放次数","Flow_NbrReqRelGnb","NUMBER","gNB请求释放的Flow数","Flow.NbrReqRelGnb"]
["正常的gNB请求释放的Flow数",null,"gnb发起的qosflow正常释放次数","Flow_NbrReqRelGnb_Normal","NUMBER","正常的gNB请求释放的Flow数","Flow.NbrReqRelGnb.Normal"]
["切出接纳失败的Flow数",null,null,"Flow_HoAdmitFail","NUMBER","切出接纳失败的Flow数","Flow.HoAdmitFail"]
["遗留Flow个数",null,null,"Flow_NbrLeft","NUMBER","遗留Flow个数","Flow.NbrLeft"]
["切换入Flow数",null,null,"Flow_NbrHoInc","NUMBER","切换入Flow数","Flow.NbrHoInc"]
["RRC连接重建请求次数",null,"rrc重建请求次数","RRC_AttConnReestab","NUMBER","RRC连接重建请求次数","RRC.AttConnReestab"]
["同频切换出成功次数",null,"同频切换成功次数","HO_SuccOutIntraFreq","NUMBER","同频切换出成功次数","HO.SuccOutIntraFreq"]
["同频切换出执行请求次数",null,"同频切换请求次数","HO_AttOutExecIntraFreq","NUMBER","同频切换出执行请求次数","HO.AttOutExecIntraFreq"]
["异频切换出成功次数",null,"异频切换成功次数","HO_SuccOutInterFreq","NUMBER","异频切换出成功次数","HO.SuccOutInterFreq"]
["异频切换出执行请求次数",null,"异频切换请求次数","HO_AttOutExecInterFreq","NUMBER","异频切换出执行请求次数","HO.AttOutExecInterFreq"]
["小区下行RLC SDU丢包数",null,"下行rlc层用户面丢包数","RLC_NbrPktLossDl","NUMBER","小区下行RLC SDU丢包数","RLC.NbrPktLossDl"]
["小区下行RLC SDU发送包数",null,"下行rlc层用户面包总数sdu","RLC_NbrPktDl","NUMBER","小区下行RLC SDU发送包数","RLC.NbrPktDl"]
["上行残留错误TB数",null,"上行mac层残留错误tb数","MAC_NbrResErrTbUl","NUMBER","上行残留错误TB数","MAC.NbrResErrTbUl"]
["上行传输初始TB数",null,"上行mac层传输初始tb数","MAC_NbrInitTbUl","NUMBER","上行传输初始TB数","MAC.NbrInitTbUl"]
["下行残留错误TB数",null,"下行mac层残留错误tb数","MAC_NbrResErrTbDl","NUMBER","下行残留错误TB数","MAC.NbrResErrTbDl"]
["下行传输TB数",null,"下行mac层传输tb总数","MAC_NbrTbDl","NUMBER","下行传输TB数","MAC.NbrTbDl"]
["下行传输初始TB数",null,"下行mac层传输初始tb数","MAC_NbrInitTbDl","NUMBER","下行传输初始TB数","MAC.NbrInitTbDl"]
["双流下行传输TB数",null,"下行传输使用rank2的tb数","MAC_NbrTbDl_Rank2","NUMBER","双流下行传输TB数","MAC.NbrTbDl.Rank2"]
["3流下行传输TB数",null,"下行传输使用rank3的tb数","MAC_NbrTbDl_Rank3","NUMBER","3流下行传输TB数","MAC.NbrTbDl.Rank3"]
["4流下行传输TB数",null,"下行传输使用rank4的tb数","MAC_NbrTbDl_Rank4","NUMBER","4流下行传输TB数","MAC.NbrTbDl.Rank4"]
["QPSK模式上行传输初始TB数",null,null,"MAC_NbrInitTbUl_Qpsk","NUMBER","QPSK模式上行传输初始TB数","MAC.NbrInitTbUl.Qpsk"]
["16QAM模式上行传输初始TB数",null,null,"MAC_NbrInitTbUl_16Qam","NUMBER","16QAM模式上行传输初始TB数","MAC.NbrInitTbUl.16Qam"]
["64QAM模式上行传输初始TB数",null,null,"MAC_NbrInitTbUl_64Qam","NUMBER","64QAM模式上行传输初始TB数","MAC.NbrInitTbUl.64Qam"]
["256QAM模式上行传输初始TB数",null,null,"MAC_NbrInitTbUl_256Qam","NUMBER","256QAM模式上行传输初始TB数","MAC.NbrInitTbUl.256Qam"]
["QPSK模式下行传输初始TB数",null,null,"MAC_NbrInitTbDl_Qpsk","NUMBER","QPSK模式下行传输初始TB数","MAC.NbrInitTbDl.Qpsk"]
["16QAM模式下行传输初始TB数",null,null,"MAC_NbrInitTbDl_16Qam","NUMBER","16QAM模式下行传输初始TB数","MAC.NbrInitTbDl.16Qam"]
["64QAM模式下行传输初始TB数",null,null,"MAC_NbrInitTbDl_64Qam","NUMBER","64QAM模式下行传输初始TB数","MAC.NbrInitTbDl.64Qam"]
["256QAM模式下行传输初始TB数",null,null,"MAC_NbrInitTbDl_256Qam","NUMBER","256QAM模式下行传输初始TB数","MAC.NbrInitTbDl.256Qam"]
["上行业务信道占用PRB数",null,"小区上行业务信道prb占用总数","RRU_DtchPrbAssnUl","NUMBER","上行业务信道占用PRB数","RRU.DtchPrbAssnUl"]
["下行业务信道占用PRB数",null,"小区下行业务信道prb占用总数","RRU_DtchPrbAssnDl","NUMBER","下行业务信道占用PRB数","RRU.DtchPrbAssnDl"]
["下行PDSCH PRB可用数",null,"下行pdsch信道prb可用数","RRU_PdschPrbTot","NUMBER","下行PDSCH PRB可用数","RRU.PdschPrbTot"]
["小区MAC层传输成功的上行流量",null,"上行mac层业务流量","MAC_CpOctUl","NUMBER","小区MAC层传输成功的上行流量","MAC.CpOctUl"]
["小区MAC层传输成功的下行流量",null,"下行mac层业务流量","MAC_CpOctDl","NUMBER","小区MAC层传输成功的下行流量","MAC.CpOctDl"]
["小区用户面上行PDCP PDU字节数","上行PDCP层用户面流量","上行pdcp层用户面流量","PDCP_UpOctUl","NUMBER","小区用户面上行PDCP PDU字节数","PDCP.UpOctUl"]
["小区用户面下行PDCP PDU字节数","下行PDCP层用户面流量","下行pdcp层用户面流量","PDCP_UpOctDl","NUMBER","小区用户面下行PDCP PDU字节数","PDCP.UpOctDl"]
["小区RB上行平均干扰电平","小区上行每PRB平均干扰电平","小区上行每prb平均干扰电平","PHY_ULMeanNL_PRB","NUMBER","小区RB上行平均干扰电平","PHY_ULMeanNL_PRB"]
["小区RB上行最大干扰电平",null,"小区上行每prb最大干扰电平","PHY_ULMaxNL_PRB","NUMBER","小区RB上行最大干扰电平","PHY_ULMaxNL_PRB"]
["RRC 重定向到LTE次数",null,"5g重定向到4g的总次数","RRC_RedirectToLTE","NUMBER","RRC 重定向到LTE次数","RRC_RedirectToLTE"]
["EPS fallback RRC 重定向到LTE次数",null,"5g重定向到4g的总次数语音触发","RRC_RedirectToLTE_EpsFB","NUMBER","EPS fallback RRC 重定向到LTE次数","RRC_RedirectToLTE_EpsFB"]
["小区平均用户数",null,"rrc连接平均用户数","RRC_SAnNsaConnUserMean","NUMBER","小区平均用户数","RRC_SAnNsaConnUserMean"]
["小区最大用户数(SA和NSA)","最大用户数","rrc连接最大用户数","RRC_SAnNsaConnUserMax","NUMBER","小区最大用户数(SA和NSA)","RRC_SAnNsaConnUserMax"]
["RRC连接平均数","用户数均值","rrc连接平均用户数","RRC_ConnMean","NUMBER","RRC连接平均数","RRC_ConnMean"]
["RRC连接最大数","RRC连接最大用户数","rrc连接最大用户数","RRC_ConnMax","NUMBER","RRC连接最大数","RRC_ConnMax"]
["LACCI",null,null,"LACCI","VARCHAR2(255)","LACCI","LACCI"]
["厂商",null,"厂商名称","VENDOR","VARCHAR2(255)","厂商","VENDOR"]
["LAC",null,null,"LAC","VARCHAR2(255)","LAC","LAC"]
["CI",null,"对象编号","CI","VARCHAR2(255)","CI","CI"]
["cell_id",null,"对象编号","CELL_ID","VARCHAR2(255)","cell_id","华为：4096*lacF+ci 诺西:16384*LAC+CI"]