{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":9,"rows_kept":16,"cut":false,"hidden":false,"merged":[[5,3,5,6],[1,4,1,6],[0,0,0,6],[12,3,12,4],[5,0,5,2],[2,4,2,6],[3,2,3,6],[12,5,12,6],[1,0,4,0],[12,0,12,1],[11,5,11,6],[11,3,11,4],[11,0,11,1],[4,2,4,6]]}
["河北联通省分ESB平台防火墙策略开通申请单"]
["申请人信息","申请人姓名","王玉龙","申请日期","2023.5.17"]
[null,"申请人电话",18631112100,"申请部门","河北省云网中心"]
[null,"申请人邮箱","wangyl5740@chinaunicom.cn"]
[null,"具体用途","通过esb kafka实现移网投诉管理系统与TOP的实时通信，交互故障工单信息。\n1. 投诉管理系统-->TOP ESB作为服务端，投诉管理系统通过socket接口访问ESB一期，ESB生成TOPIC供TOP消费使用。\n2. TOP-->投诉管理系统 ESB作为服务端，TOP系统通过socket接口推送数据到ESB，ESB生成TOPIC供投诉管理系统消费使用。"]
["本端业务系统信息(源)",null,null,"需要访问的对端业务系统信息（目的）"]
["序号","系统名称","IP地址","系统名称","IP地址","掩码","端口"]
[1,"TOP","10.17.180.3","省内ESB","10.160.84.4",null,"9136-9140","socket","推送数据"]
[2,"TOP","10.17.180.3","省内ESB","10.160.84.9（承载网IP）\n10.160.84.10（承载网IP）\n10.160.84.11（承载网IP）",null,"2181和9092","kafka","从TOPIC上消费"]
[3,"河北联通移网投诉管理系统（诺基亚）","172.16.110.3（ESB一期地址）\n172.16.110.4（ESB一期地址）\n172.16.110.7（ESB一期地址）\n172.16.110.41（ESB一期地址）\n172.16.110.42（ESB一期地址）","省内ESB","10.160.84.4",null,"9136-9140","socket","推送数据"]
[4,"河北联通移网投诉管理系统（诺基亚）","172.16.110.3（ESB一期地址）\n172.16.110.4（ESB一期地址）\n172.16.110.7（ESB一期地址）\n172.16.110.41（ESB一期地址）\n172.16.110.42（ESB一期地址）","省内ESB","10.160.84.9（承载网IP）\n10.160.84.10（承载网IP）\n10.160.84.11（承载网IP）",null,"2181和9092","kafka","从TOPIC上消费"]
["申请部门领导意见",null,null,"申请部门领导（签字）"]
["管理部门领导意见",null,null,"管理部门领导（签字）"]
[]
[]
[{"$nulls":4},"          申请人签字："]